/**
  @page STM32100B_EVAL_Binary UM0891 STM32100B-EVAL Binary files Readme file
  
  @verbatim
  ******************** (C) COPYRIGHT 2011 STMicroelectronics *******************
  * @file    STM32100B-EVAL/Binary/readme.txt 
  * @author  MCD Application Team
  * @version V1.1.0
  * @date    08-April-2011
  * @brief   Description of the UM0891 "STM32100B-EVAL demonstration firmware" 
  *          Binary files.
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
   @endverbatim

@par Description

This directory contains a set of STM32100B-EVAL Demo binary files that should be
programmed to the internal FLASH using different methods: 
   - In-Circuit-Programming using the embedded bootloader
   - In-Application-Programming through USART

 - Using Bootloader:
    - To program the demonstration's binary image into the internal Flash memory,
      you have to use the "stm32100b_eval_fw_v1.1.0.bin" file located under 
      Project\STM32100B-EVAL\Binary with embedded Bootloader. 
      For more details, please refer to Bootloader application note AN2606 
      STM32 microcontroller system memory boot mode.   

 - Using IAP:
    - To program the demonstration's binary image into the internal Flash memory,
      you have to use the "stm32100b-eval_fw_v1.1.0_offset_0x3000.bin" file 
      located under Project\STM32100B-EVAL\Binary with IAP over USART. For more 
      details, please refer to IAP application note AN2557 STM32F10x in-application 
      programming using the USART. 
    
@note
 - Low-density Value line devices are STM32F100xx microcontrollers where the 
   Flash memory density ranges between 16 and 32 Kbytes.
 - Low-density devices are STM32F101xx, STM32F102xx and STM32F103xx 
   microcontrollers where the Flash memory density ranges between 16 and 32 Kbytes.
 - Medium-density Value line devices are STM32F100xx microcontrollers where
   the Flash memory density ranges between 64 and 128 Kbytes.  
 - Medium-density devices are STM32F101xx, STM32F102xx and STM32F103xx 
   microcontrollers where the Flash memory density ranges between 64 and 128 Kbytes.
 - High-density Value line devices are STM32F100xx microcontrollers where
   the Flash memory density ranges between 256 and 512 Kbytes.
 - High-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 256 and 512 Kbytes.
 - XL-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 512 and 1024 Kbytes.
 - Connectivity line devices are STM32F105xx and STM32F107xx microcontrollers.
 
 * <h2><center>&copy; COPYRIGHT 2011 STMicroelectronics</center></h2>
 */
