/**
  @page WFE_Stop_Flash AN2629 WFE_Stop_Flash Readme file
  
  @verbatim
  ******************** (C) COPYRIGHT 2009 STMicroelectronics *******************
  * @file WFE_Stop_Flash/readme.txt 
  * @author   MCD Application Team
  * @version  V2.0.0
  * @date     04/27/2009
  * @brief    Description of the AN2629 Application note's WFE_Stop_Flash.
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
   @endverbatim

@par Example Description 

This example describes how to use the Wait for Event instruction and the Stop mode 
of the STM32F10xxx, using the firmware found in the Zip file delivered with this 
application note. 
WFE_Stop_Flash example is strictly mapped in the Flash memory and runs from the 
Flash memory.

@par Directory contents 

   
    - inc 
       - WFE_Stop_Flash/inc/stm32f10x_conf.h     Library Configuration file 
       - WFE_Stop_Flash/inc/stm32f10x_it.h       Interrupt handlers header file 

    - src 
      - WFE_Stop_Flash/src/stm32f10x_it.c        Interrupt handlers 
      - WFE_Stop_Flash/src/main.c                Main program file
  
   
@par Hardware and Software environment  

  - This example runs on STM32F10x High-Density, STM32F10x Medium-Density and
    STM32F10x Low-Density Devices.
  
  - This example has been tested with STMicroelectronics STM3210B-EVAL  evaluation 
    boards and can be easily tailored to any other supported device and development 
    board.
   
  
  - STM3210B-EVAL Set-up 
  
    - Use this example with STM32F10xxx evaluation board: refer to the user manual UM0426:
     “STM3210B-EVAL evaluation board” to use the STM3210B-EVAL.
    - After connecting the power supply and the JTAG tools, the power consumption 
      can be measured by replacing Jumper JP9 by an ampermeter.
            
         
@par How to use it ? 

In order to load the WFE_Stop_Flash code, you have do the following:

  - RVMDK 
    - Open the WFE_Stop_Flash.uv2 project
    - Rebuild all files: Project->Rebuild all target files
    - Load project image: Debug->Start/Stop Debug Session
    - Run program: Debug->Run (F5)

  - RIDE 
    - Open the WFE_Stop_Flash.rprj project
    - Rebuild all files: Project->Build Project
    - Load project image: Debug->start
    - Run program: Debug->Run(ctrl+F9)  
    
  - EWARMv5 
    - Open the WFE_Stop_Flash.eww workspace.
    - Rebuild all files: Project->Rebuild all
    - Load project image: Project->Debug
    - Run program: Debug->Go(F5)

@note
 - Low-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 16 and 32 Kbytes.
 - Medium-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 32 and 128 Kbytes.
 - High-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 256 and 512 Kbytes.

 * <h2><center>&copy; COPYRIGHT 2009 STMicroelectronics</center></h2>
 */
