/**
  @page tasking TASKING Project Template for STM32F2xx devices
 
  @verbatim
  ******************** (C) COPYRIGHT 2011 STMicroelectronics *******************
  * @file    readme.txt
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    19-August-2011
  * @brief   This sub-directory contains all the user-modifiable files needed to
  *          create a new project linked with the STM32F2xx Standard Peripherals
  *          Library and working with TASKING VX-toolset for ARM Cortex-M V3.2r1.
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
  * AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
  * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
  * CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
  * INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
  @endverbatim
 
 @par Directory contents
 
 - .cproject/.project: A pre-configured project file with the provided library
                       structure that produces an executable image with TASKING.

- TASKING                     : This folder contains
 
     - stm32f2xx.lsl          : This file is TASKING linker script that contains the 
                                STM32F2xx vector table and used to place program code (readonly) 
                                in internal FLASH and data (readwrite, Stack and Heap)in
                                internal SRAM. 
                                You can customize this file to your need.

     - cstart_thumb2.asm      : This file initializes the stack pointer and copy initialized
                                sections from ROM to RAM
                           
 @par How to use it ?

 - Open TASKING toolchain.
 - Click on File->Import, select General->'Existing Projects into Workspace' 
   and then click "Next". 
 - Browse to  TASKING workspace directory and select the project: 
   - STM322xG-EVAL: to configure the project for STM32F2xx devices.
 - Under Windows->Preferences->General->Workspace->Linked Resources, add 
   a variable path named "Cur_Path" which points to the folder containing
   "Libraries", "Project" and "Utilities" folders.
 - Rebuild all project files: Select the project in the "Project explorer" 
   window then click on Project->build project menu.
 - Run program: Select the project in the "Project explorer" window then click 
   Run->Debug (F11)

 @note The needed define symbols for this config are already declared in the
       preprocessor section: USE_STM322xG_EVAL, STM32F2XX, USE_STDPERIPH_DRIVER 

 * <h3><center>&copy; COPYRIGHT 2011 STMicroelectronics</center></h3>
 */
