| CMSIS-CORE Version 3.00 CMSIS-CORE support for Cortex-M processor-based devices

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Usage and Description
- Reference

Register Mapping

The table below associates some common register names used in CMSIS to the register names used in Technical Reference Manuals.

CMSIS Register Name | Cortex-M3 and Cortex-M4 | Cortex-M0 | Register Name
--- | --- | --- | ---
Nested Vectored Interrupt Controller (NVIC) Register Access
NVIC->ISER[] | NVIC_ISER0..7 | ISER | Interrupt Set-Enable Registers
NVIC->ICER[] | NVIC_ICER0..7 | ICER | Interrupt Clear-Enable Registers
NVIC->ISPR[] | NVIC_ISPR0..7 | ISPR | Interrupt Set-Pending Registers
NVIC->ICPR[] | NVIC_ICPR0..7 | ICPR | Interrupt Clear-Pending Registers
NVIC->IABR[] | NVIC_IABR0..7 | - | Interrupt Active Bit Register
NVIC->IP[] | NVIC_IPR0..59 | IPR0..7 | Interrupt Priority Register
NVIC->STIR | STIR | - | Software Triggered Interrupt Register
System Control Block (SCB) Register Access
SCB->CPUID | CPUID | CPUID | CPUID Base Register
SCB->ICSR | ICSR | ICSR | Interrupt Control and State Register
SCB->VTOR | VTOR | - | Vector Table Offset Register
SCB->AIRCR | AIRCR | AIRCR | Application Interrupt and Reset Control Register
SCB->SCR | SCR | SCR | System Control Register
SCB->CCR | CCR | CCR | Configuration and Control Register
SCB->SHP[] | SHPR1..3 | SHPR2..3 | System Handler Priority Registers
SCB->SHCSR | SHCSR | SHCSR | System Handler Control and State Register
SCB->CFSR | CFSR | - | Configurable Fault Status Registers
SCB->HFSR | HFSR | - | HardFault Status Register
SCB->DFSR | DFSR | - | Debug Fault Status Register
SCB->MMFAR | MMFAR | - | MemManage Fault Address Register
SCB->BFAR | BFAR | - | BusFault Address Register
SCB->AFSR | AFSR | - | Auxiliary Fault Status Register
SCB->PFR[] | ID_PFR0..1 | - | Processor Feature Registers
SCB->DFR | ID_DFR0 | - | Debug Feature Register
SCB->ADR | ID_AFR0 | - | Auxiliary Feature Register
SCB->MMFR[] | ID_MMFR0..3 | - | Memory Model Feature Registers
SCB->ISAR[] | ID_ISAR0..4 | - | Instruction Set Attributes Registers
SCB->CPACR | CPACR | - | Coprocessor Access Control Register
System Control and ID Registers not in the SCB (SCnSCB) Register Access
SCnSCB->ICTR | ICTR | - | Interrupt Controller Type Register
SCnSCB->ACTLR | ACTLR | - | Auxiliary Control Register
System Timer (SysTick) Control and Status Register Access
SysTick->CTRL | STCSR | SYST_CSR | SysTick Control and Status Register
SysTick->LOAD | STRVR | SYST_RVR | SysTick Reload Value Register
SysTick->VAL | STCVR | SYST_CVR | SysTick Current Value Register
SysTick->CALIB | STCR | SYST_CALIB | SysTick Calibaration Value Register
Data Watchpoint and Trace (DWT) Register Access
DWT->CTRL | DWT_CTRL | - | Control Register
DWT->CYCCNT | DWT_CYCCNT | - | Cycle Count Register
DWT->CPICNT | DWT_CPICNT | - | CPI Count Register
DWT->EXCCNT | DWT_EXCCNT | - | Exception Overhead Count Register
DWT->SLEEPCNT | DWT_SLEEPCNT | - | Sleep Count Register
DWT->LSUCNT | DWT_LSUCNT | - | LSU Count Register
DWT->FOLDCNT | DWT_FOLDCNT | - | Folded-instruction Count Register
DWT->PCSR | DWT_PCSR | - | Program Counter Sample Register
DWT->COMP0..3 | DWT_COMP0..3 | - | Comparator Register 0..3
DWT->MASK0..3 | DWT_MASK0..3 | - | Mask Register 0..3
DWT->FUNCTION0..3 | DWT_FUNCTION0..3 | - | Function Register 0..3
Instrumentation Trace Macrocell (ITM) Register Access
ITM->PORT[] | ITM_STIM0..31 | - | Stimulus Port Registers
ITM->TER | ITM_TER | - | Trace Enable Register
ITM->TPR | ITM_TPR | - | ITM Trace Privilege Register
ITM->TCR | ITM_TCR | - | Trace Control Register
Trace Port Interface (TPIU) Register Access
TPI->SSPSR | TPIU_SSPR | - | Supported Parallel Port Size Register
TPI->CSPSR | TPIU_CSPSR | - | Current Parallel Port Size Register
TPI->ACPR | TPIU_ACPR | - | Asynchronous Clock Prescaler Register
TPI->SPPR | TPIU_SPPR | - | Selected Pin Protocol Register
TPI->FFSR | TPIU_FFSR | - | Formatter and Flush Status Register
TPI->FFCR | TPIU_FFCR | - | Formatter and Flush Control Register
TPI->FSCR | TPIU_FSCR | - | Formatter Synchronization Counter Register
TPI->TRIGGER | TRIGGER | - | TRIGGER
TPI->FIFO0 | FIFO data 0 | - | Integration ETM Data
TPI->ITATBCTR2 | ITATBCTR2 | - | ITATBCTR2
TPI->ITATBCTR0 | ITATBCTR0 | - | ITATBCTR0
TPI->FIFO1 | FIFO data 1 | - | Integration ITM Data
TPI->ITCTRL | TPIU_ITCTRL | - | Integration Mode Control
TPI->CLAIMSET | CLAIMSET | - | Claim tag set
TPI->CLAIMCLR | CLAIMCLR | - | Claim tag clear
TPI->DEVID | TPIU_DEVID | - | TPIU_DEVID
TPI->DEVTYPE | TPIU_DEVTYPE | - | TPIU_DEVTYPE
Memory Protection Unit (MPU) Register Access
MPU->TYPE | MPU_TYPE | - | MPU Type Register
MPU->CTRL | MPU_CTRL | - | MPU Control Register
MPU->RNR | MPU_RNR | - | MPU Region Number Register
MPU->RBAR | MPU_RBAR | - | MPU Region Base Address Register
MPU->RASR | MPU_RASR | - | MPU Region Attribute and Size Register
MPU->RBAR_A1..3 | MPU_RBAR_A1..3 | - | MPU alias Register
MPU->RSAR_A1..3 | MPU_RSAR_A1..3 | - | MPU alias Register
Floating Point Unit (FPU) Register Access [only Cortex-M4 with FPU]
FPU->FPCCR | FPCCR | - | FP Context Control Register
FPU->FPCAR | FPCAR | - | FP Context Address Register
FPU->FPDSCR | FPDSCR | - | FP Default Status Control Register
FPU->MVFR0..1 | MVFR0..1 | - | Media and VFP Feature Registers