Back to Release page
# Release Notes for STM32L152_EVAL Evaluation Board Drivers Copyright 2012 STMicroelectronics
## Contents STM32L152_EVAL Evaluation Board Drivers update History License ## STM32L152_EVAL Evaluation Board Drivers update History ### V5.0.2 / 09-March-2012 Main Changes All source files: license disclaimer text update and add link to the License file on ST Internet. stm32l152_eval.c In sEE_LowLevel_Init() and LM75_LowLevel_Init() functions: swap the order of I2C IOs and alternate function (AF) configuration (AF configuration should be done before to configure the IOs). ### V5.0.1 / 24-January-2012 Main Changes All source files: update disclaimer to add reference to the new license agreement stm32l152_eval.c and stm32l152_eval_lcd.h/.c Fix some strict ANSI-C errors. ### V5.0.0 / 02-December-2011 Main Changes Update STM32 Evaluation Board Drivers architecture and folder organization, full API compatibility maintained vs. V4.6.2 All the HW drivers required for each board are provided within this board folder. The concerned drivers are: stm32_eval_i2c_ee.c\.h: I2C M24Cxx EEPROM memory driver stm32_eval_i2c_tsensor.c\.h: I2C LM75 temperature sensor driver stm32_eval_spi_flash.c\.h: SPI M25Pxxx FLASH memory driver stm32_eval_sdio_sd.c\.h: SDIO SD Card memory driver stm32_eval_spi_sd.c\.h: SPI SD Card memory driver These drivers were moved from \Common to \STM32XXX_EVAL folder(s) \Common folder contains only drivers for the fonts and log module used by the LCD driver stm32_eval.c\.h files removed, as consequence you need to perform the following update on your project configuration (based on EVAL drivers V4.6.2): In the project files, add your EVAL board driver source file (ex. "stm32l152_eval.c") instead of "stm32_eval.c" Include your EVAL board driver header file (ex. #include "stm32l152_eval.h") instead of #include "stm32_eval.h" If you are using the EVAL board's LCD, you need to add the include of the LCD header file (ex: #include "stm32l152_eval_lcd.h") If you are using the LCD log module, after copying it to the application folder you have to edit it and update the name of the LCD header file. For more details, refer to the lcd_log_conf_template.h driver description. stm32l152_eval_lcd.c: update to support new LCD AM240320D5TOQW01H (controller ILI9325) ### V4.6.2 / 22-July-2011 Main Changes STM3210C_EVAL stm3210c_eval_lcd.c: update to support new LCD AM240320D5TOQW01H (controller ILI9325) STM322xG-EVAL stm322xg_eval.h: fix value of the SDIO clock divider (SDIO_TRANSFER_CLK_DIV constant) to 2 instead of 0 stm322xg_eval_lcd.c: increase FSMC AddressSetupTime value from 1 to 3 to be compliant with some LCD access timing stm322xg_eval_audio_codec.c: update Codec_CtrlInterface_Init() and Codec_GPIO_Init() functions to not reconfigure the I2C peripheral if it's already enabled and configured (to avoid configuring the I2C twice when using both Audio codec and IO Expander drivers in the same application). ### V4.6.1 / 18-April-2011 Main Changes Update some STM322xG_EVAL drivers (no change on the API) to fix warnings with TASKING C compiler. Change the Release Notes name to STM32 Evaluation Board Drivers stm322xg_eval.c SD_LowLevel_Init(): change SDIO pins speed configuration to "GPIO_Speed_25MHz" ### V4.6.0 / 11-March-2011 Main Changes Official version supporting STM322xG_EVAL evaluation board RevB (for STM32F2xx devices). Common Add new LCD log utility drivers: The LCD Log module allows to automatically set a header and footer on any application using the LCD display and allows to dump user, debug and error messages by using the following macros: LCD_ErrLog(), LCD_UsrLog() and LCD_DbgLog(). Note: the STM322xG_EVAL board RevA was wrongly named STM3220F_EVAL ### V4.5.0 / 07-March-2011 Main Changes stm32_eval_sdio_sd.c\.h: driver improvement SD Clock increased to 24MHz to improve the data transfer performance. Add new functions to check the SDIO peripheral and SD Card status at any time: SD_WaitReadOperation(), SD_WaitWriteOperation(). The software sequence is little bit changed but without any impact on driver API. For more details, refer to the stm32_eval_sdio_sd.c driver description. Add new structure containing the SD Status register parameters. This structure is called by the SD_SendSDStatus() function. Transfers mode updated Read/Write Block using Polling and DMA modes Read/Write Multi Blocks using DMA mode only Interrupt mode removed Data transfer functions are managing only fixed Block size (512-byte) STM32100B-EVAL stm32100b_eval_cec.c: fix some strict ANSI-C errors STM32100E-EVAL stm32100e_eval_cec.c: fix some strict ANSI-C errors ### V4.4.0 / 31-December-2010 Main Changes Add new directory for STM32L152-EVAL board containing the following files: stm32l152_eval.h/.c, stm32l152_eval_lcd.h/.c, stm32l152_eval_glass_lcd.h/.c, stm32l152_eval_i2c_ee.h/.c Add support for the STM32100E-EVAL Rev B: SPI FLASH CS pin "sFLASH_CS_PIN" changed from PB.02 to PE.06. stm32100e_eval_lcd.h/.c: Add support for "LCD_ILI9325" LCD controller. stm32100e_eval_fsmc_onenand.h/.c driver updated to correct asynchronous and synchronous read operations procedures. ### 4.3.0 - 10/15/2010 General I2C EEPROM, Temperature Sensor and IOE Expander drivers updated to use the DMA for read/write transfer and add more robustness SD Card (SDIO) driver updated to add more robustness SPI Flash and SD Card (SPI) drivers: SPI MISO pin configuration changed to Input Floating Utilities Add new directory for STM32100E-EVAL board containing the following files: stm32100e_eval.h/.c, stm32100e_eval_lcd.h/.c, stm32100e_eval_cec.h/.c, stm32100e_eval_fsmc_onenand.h/.c, stm32100e_eval_fsmc_sram.h/.c, stm32100e_eval_ioe.h/.c Common stm32_eval_sdio_sd.c: Update the DMA End of Transfer Check loop inside the SD_ReadBlock(), SD_WriteBlock(), SD_ReadMultiBlocks() and SD_Write MultiBlocks(). stm32_eval_i2c_ee.c/.h Enhanced sEE_WaitEepromStandbyState() function for more robustness. Enhanced Read and Write operations to manage I2C limitations. Add Timeout management with user callback implementation which allows recovering from I2C bus errors. Add critical sections user callbacks allowing to disable then enable interrupts when I2C operation require to be not interrupted. stm32_eval_i2c_tsensor.c/.h Enhanced I2C communication functions by using DMA for registers Read and Write operations. Add Timeout management with user callback implementation which allows recovering from I2C bus errors. STM32100B_EVAL stm32100b_eval.h: Add LM75 DMA defines. stm32100b_eval_lcd.c: Change "SPI_FLASH" by "sFLASH" in LCD_DrawBMP() function. STM3210B_EVAL stm3210b_eval.h: Add LM75 DMA defines. stm3210b_eval_lcd.c: Change "SPI_FLASH" by "sFLASH" in LCD_DrawBMP() function. STM3210C_EVAL stm3210c_eval.h: Add EEPROM driver Timeout define. stm3210c_eval_lcd.c: Change "SPI_FLASH" by "sFLASH" in LCD_DrawBMP() function. stm3210c_eval_i2c_ioe.c Enhanced I2C communication functions by using DMA for registers Read and Write operations. Add Timeout management with user callback implementation which allows recovering from I2C bus errors. change IOE_I2C_SPEED from "400000" to "300000". STM3210E_EVAL stm3210e_eval.c: change "void SD_WaitForDMAEndOfTransfer(void)" to "uint32_t SD_DMAEndOfTransferStatus(void)". stm3210e_eval.h: Add LM75 DMA defines. stm3210e_eval_fsmc_nand.h: remove "NAND_CMD_AREA_TRUE1" define. stm3210e_eval_fsmc_nand.c: Update FSMC timing in NAND_Init() function to be aligned with AN2784 application note. stm3210e_eval_fsmc_nor.c NOR_Init() function: add FSMC_AsynchronousWait field to FSMC_NORSRAMInitStructure stm3210e_eval_fsmc_sram.c Update FSMC timing in SRAM_Init() function to be aligned with AN2784 application note. SRAM_Init() function: add FSMC_AsynchronousWait field to FSMC_NORSRAMInitStructure stm3210e_eval_lcd.c LCD_FSMCConfig() function: add FSMC_AsynchronousWait field to FSMC_NORSRAMInitStructure ### 4.2.0 - 04/16/2010 General I2C EEPROM driver update to use the DMA to perform data transfer to/from EEPROM memory. Utilities STM32_EVAL stm32_eval_i2c_ee.c: updated to use the DMA to perform data transfer to/from EEPROM memory. For more details, refer to the description provided within this file. stm3210c_eval.c: add low level functions to configure the DMA (needed for I2C EEPROM driver) stm3210c_eval_ioe.c: add a delay in IOE_TS_GetState() function to wait till the end of ADC conversion stm3210e_eval_fsmc_nor.c: add PD6 pin configuration in NOR_Init() function stm3210b_eval_lcd.c: remove the second ";" from "static void PutPixel(int16_t x, int16_t y);;" ### 4.1.0 - 03/01/2010 General Add support for STM32 Low-density Value line (STM32F100x4/6) and Medium-density Value line (STM32F100x8/B) devices. Add support for the STMicroelectronics STM32100B-EVAL evaluation board. Utilities STM32_EVAL Add new directory "Common" containing a common drivers for all STM32 evaluation boards: fonts.h/.c, stm32_eval_i2c_ee.h/.c, stm32_eval_spi_flash.h/.c, stm32_eval_i2c_tsensor.h/.c, stm32_eval_spi_sd.h/.c and stm32_eval_sdio_sd.h/.c Add new driver for the STM32100B-EVAL managing Leds, push button and COM ports. New HDMI CEC High level driver. For all LCD drivers new fonts has been added. New FSMC memories drivers for STM3210E-EVAL board: stm3210e_eval_fsmc_sram.h/.c, stm3210e_eval_fsmc_nor.h/.c and stm3210e_eval_fsmc_nand.h/.c. ## License Licensed under MCD-ST Liberty SW License Agreement V2, (the "License"); You may not use this package except in compliance with the License. You may obtain a copy of the License at: http://www.st.com/software_license_agreement_liberty_v2 Unless required by applicable law or agreed to in writing, software distributed under the License is distributed on an "AS IS" BASIS, WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied. See the License for the specific language governing permissions and limitations under the License. For complete documentation on STM32 Microcontrollers visit www.st.com/STM32