/**
  @page exampletemplate Project Example Template
  
  @verbatim
  ******************** (C) COPYRIGHT 2012 STMicroelectronics *******************
  * @file    readme.txt 
  * @author  MCD Application Team
  * @version V1.1.1
  * @date    13-April-2012
  * @brief   This sub-directory contains all the user-modifiable files 
  *          needed to create a new project linked with the STM32L1xx  
  *          Standard Peripheral Library.
  ******************************************************************************
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
   @endverbatim

@par Project Example Template Description 

This example is used as a template that can be used as refrence to build any new 
firmware development for STM32L1xx Ultra Low Power Medium- and High-density 
devices using the STM32L1xx Standard Peripherals Library.


@par Directory contents 

This folder contains standard template projects for EWARM, TASKING, MDK-ARM, RIDE
and TrueSTUDIO toolchains that compile the needed STM32L1xx Standard Peripheral's 
drivers plus all the user-modifiable files that are necessary to create a new 
project. 

  - Project/STM32L1xx_StdPeriph_Templates/stm32l1xx_conf.h    Library Configuration file

  - Project/STM32L1xx_StdPeriph_Templates/stm32l1xx_it.c:     Source file containing the interrupt handlers (the 
                                                              function bodies are empty in this template).

  - Project/STM32L1xx_StdPeriph_Templates/stm32l1xx_it.h      Header file including all interrupt handlers prototypes.

  - Project/STM32L1xx_StdPeriph_Templates/main.c              Main program
  
  - Project/STM32L1xx_StdPeriph_Templates/main.h              Header file for Main program  

  - Project/STM32L1xx_StdPeriph_Templates/system_stm32l1xx.c  
          The "system_stm32l1xx.c" is generated by an automatic clock configuration 
          system and can be easily customized to your own configuration.
          To select different clock setup, use the "STM32L1xx_Clock_Configuration_V1.1.0.xls" 
          provided with the AN3309 package available on <a href="http://www.st.com/internet/mcu/family/141.jsp">  ST Microcontrollers </a>
        
@note
- Ultra Low Power Medium-density devices are STM32L151xx and STM32L152xx 
  microcontrollers where the Flash memory density ranges between 64 and 128 Kbytes.
- Ultra Low Power Medium-density Plus devices are STM32L151xx, STM32L152xx and 
  STM32L162xx microcontrollers where the Flash memory density is 256 Kbytes.
- Ultra Low Power High-density devices are STM32L151xx, STM32L152xx and STM32L162xx 
  microcontrollers where the Flash memory density is 384 Kbytes.

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */


