/******************** (C) COPYRIGHT 2006 STMicroelectronics ********************
* File Name          : Readme.txt
* Author             : MCD Application Team
* Date First Issued  : 03/10/2006
* Description        : Describes how to load the "STR750_Speech.wav", "OSIRIS.wav"  
*                      and "Alarm.wav" files in the M25P64 SPI FLASH memory mounted 
*                      on the STR75x-EVAL board.
********************************************************************************
* History:
* 07/17/2006 : V1.0
* 03/10/2006 : V0.1 
********************************************************************************
* THE PRESENT SOFTWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH SOFTWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

The M25P64 SPI FLASH memory is connected to the Serial memory interface (SMI) 
Bank0; it is seen by the CPU as memory mapped in AHB address (at @0x80000000).
This memory is used in the STR75x-EVAL demonstration to store the "OSIRIS.wav", 
"STR750_Speech.wav" and "Alarm.wav" files.

In order to store these files in the M25P64 memory, use your toolchain to:
 - Load "STR750_Speech.wav" file into memory starting from address 0x80100000 
 - Load "OSIRIS.wav" file into memory starting from address 0x80400000
 - Load "Alarm.wav" file into memory starting from address 0x80600000

******************* (C) COPYRIGHT 2006 STMicroelectronics *****END OF FILE****
