| CMSIS-CORE Version 3.00 CMSIS-CORE support for Cortex-M processor-based devices

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

Data Fields
IPSR_Type Union Reference

Union type to access the Interrupt Program Status Register (IPSR).

## Data Fields
struct {
uint32_t ISR:9
| bit: 0.. 8 Exception number
uint32_t _reserved0:23
| bit: 9..31 Reserved
} | b
| Structure used for bit access.
uint32_t | w
| Type used for word access.